From 554fd8c5195424bdbcabf5de30fdc183aba391bd Mon Sep 17 00:00:00 2001
From: upstream source tree <ports@midipix.org>
Date: Sun, 15 Mar 2015 20:14:05 -0400
Subject: obtained gcc-4.6.4.tar.bz2 from upstream website; verified
 gcc-4.6.4.tar.bz2.sig; imported gcc-4.6.4 source tree from verified upstream
 tarball.

downloading a git-generated archive based on the 'upstream' tag
should provide you with a source tree that is binary identical
to the one extracted from the above tarball.

if you have obtained the source via the command 'git clone',
however, do note that line-endings of files in your working
directory might differ from line-endings of the respective
files in the upstream repository.
---
 gcc/config/m68k/m68k-modes.def | 25 +++++++++++++++++++++++++
 1 file changed, 25 insertions(+)
 create mode 100644 gcc/config/m68k/m68k-modes.def

(limited to 'gcc/config/m68k/m68k-modes.def')

diff --git a/gcc/config/m68k/m68k-modes.def b/gcc/config/m68k/m68k-modes.def
new file mode 100644
index 000000000..06297cad9
--- /dev/null
+++ b/gcc/config/m68k/m68k-modes.def
@@ -0,0 +1,25 @@
+/* M68k extra machine modes. 
+   Copyright (C) 2003, 2004, 2007 Free Software Foundation, Inc.
+
+This file is part of GCC.
+
+GCC is free software; you can redistribute it and/or modify
+it under the terms of the GNU General Public License as published by
+the Free Software Foundation; either version 3, or (at your option)
+any later version.
+
+GCC is distributed in the hope that it will be useful,
+but WITHOUT ANY WARRANTY; without even the implied warranty of
+MERCHANTABILITY or FITNESS FOR A PARTICULAR PURPOSE.  See the
+GNU General Public License for more details.
+
+You should have received a copy of the GNU General Public License
+along with GCC; see the file COPYING3.  If not see
+<http://www.gnu.org/licenses/>.  */
+
+/* These differ in the representation of the canonical NaN.  */
+RESET_FLOAT_FORMAT (SF, motorola_single_format);
+RESET_FLOAT_FORMAT (DF, motorola_double_format);
+
+/* 80-bit floating point (IEEE extended, in a 96-bit field) */
+FRACTIONAL_FLOAT_MODE (XF, 80, 12, ieee_extended_motorola_format);
-- 
cgit v1.2.3

