<html><head><meta name="color-scheme" content="light dark"></head><body><pre style="word-wrap: break-word; white-space: pre-wrap;">/* m68k device names -*- C -*-
   Copyright (C) 2005, 2006, 2007, 2008 Free Software Foundation, Inc.
   Written by CodeSourcery

   This file is part of GCC.

   GCC is free software; you can redistribute it and/or modify it
   under the terms of the GNU General Public License as published by
   the Free Software Foundation; either version 3, or (at your option)
   any later version.

   GCC is distributed in the hope that it will be useful, but
   WITHOUT ANY WARRANTY; without even the implied warranty of
   MERCHANTABILITY or FITNESS FOR A PARTICULAR PURPOSE.  See the GNU
   General Public License for more details.

   You should have received a copy of the GNU General Public License
   along with GCC; see the file COPYING3.  If not see
   &lt;http://www.gnu.org/licenses/&gt;.  */

/* This file lists each target device that we support.  It is used by
   both C code and build scripts.

   Following Freescale's lead, we group devices into families that share
   the same core and extension units.  Devices in these families differ
   only in the set of peripherals they provide.  We pick one device to
   act as the representative of each family.

   We further group device families into multilibs, again picking one
   family (and its representative device) to represent each multilib.

   Devices are declared using the construct:

      M68K_DEVICE (NAME, ENUM_VALUE, FAMILY, MULTILIB, MICROARCH, ISA, FLAGS)

   where the arguments are as follows:

      NAME
	The name of the device as a string.  This string acts as the
	device's -mcpu argument and is guaranteed to be unique.

      ENUM_VALUE
	The associated value in the target_device enumeration.
	This value is also guaranteed to be unique.

      FAMILY
	The NAME field of the family's representative device.

      MULTILIB
	The NAME field of the multilib's representative device.

      MICROARCH
	The class of core used by devices in this family.  The field
	is a uarch enumeration value without the leading "u".

      ISA
	The ISA implemented by this family.  The field is
	an m68k_isa enumeration value.

      FLAGS
	The FL_* flags that apply to this family, excluding FL_FOR_isa_*.
	See m68k.h for the full list.

   There is a bit of duplication between devices in the same family,
   but this approach makes scripting easier.  We keep each entry on
   a single line for the same reason.

   As the compiler does not (currently) generate MAC or EMAC commands,
   we do not need separate multilibs for cores that only differ in
   their MAC functionality.  */

/* 680x0 series processors.  */
M68K_DEVICE ("68000", m68000,   "68000", "68000", 68000,    isa_00,    0)
M68K_DEVICE ("68010", m68010,   "68010", "68000", 68010,    isa_10,    0)
M68K_DEVICE ("68020", m68020,   "68020", "68020", 68020,    isa_20,    FL_MMU | FL_UCLINUX)
M68K_DEVICE ("68030", m68030,   "68030", "68020", 68030,    isa_20,    FL_MMU | FL_UCLINUX)
M68K_DEVICE ("68040", m68040,   "68040", "68040", 68040,    isa_40,    FL_MMU)
M68K_DEVICE ("68060", m68060,   "68060", "68060", 68060,    isa_40,    FL_MMU)
M68K_DEVICE ("68302", m68302,   "68302", "68000", 68000,    isa_00,    FL_MMU)
M68K_DEVICE ("68332", m68332,   "68332", "cpu32", cpu32,    isa_cpu32, FL_MMU)
M68K_DEVICE ("cpu32", cpu32,    "cpu32", "cpu32", cpu32,    isa_cpu32, FL_MMU)

/* ColdFire CFV1 processor.  */
/* For historical reasons, the 51 multilib is named 51qe.  */
M68K_DEVICE ("51",    mcf51,    "51",    "51qe",  cfv1,     isa_c,     FL_CF_USP)
M68K_DEVICE ("51ac",  mcf51ac,  "51",    "51qe",  cfv1,     isa_c,     FL_CF_USP)
M68K_DEVICE ("51cn",  mcf51cn,  "51",    "51qe",  cfv1,     isa_c,     FL_CF_USP)
M68K_DEVICE ("51em",  mcf51em,  "51",    "51qe",  cfv1,     isa_c,     FL_CF_USP | FL_CF_MAC)
M68K_DEVICE ("51jm",  mcf51jm,  "51",    "51qe",  cfv1,     isa_c,     FL_CF_USP)
M68K_DEVICE ("51qe",  mcf51qe,  "51",    "51qe",  cfv1,     isa_c,     FL_CF_USP)

/* ColdFire CFV2 processors.  */
M68K_DEVICE ("5202",  mcf5202,  "5206",  "5206",  cfv2,     isa_a,     0)
M68K_DEVICE ("5204",  mcf5204,  "5206",  "5206",  cfv2,     isa_a,     0)
M68K_DEVICE ("5206",  mcf5206,  "5206",  "5206",  cfv2,     isa_a,     0)
M68K_DEVICE ("5206e", mcf5206e, "5206e", "5206e", cfv2,     isa_a,     FL_CF_HWDIV | FL_CF_MAC)
M68K_DEVICE ("5207",  mcf5207,  "5208",  "5208",  cfv2,     isa_aplus, FL_CF_HWDIV | FL_CF_EMAC)
M68K_DEVICE ("5208",  mcf5208,  "5208",  "5208",  cfv2,     isa_aplus, FL_CF_HWDIV | FL_CF_EMAC)
M68K_DEVICE ("5210a", mcf5210a, "5211a", "5208",  cfv2,     isa_aplus, FL_CF_HWDIV | FL_CF_MAC)
M68K_DEVICE ("5211a", mcf5211a, "5211a", "5208",  cfv2,     isa_aplus, FL_CF_HWDIV | FL_CF_MAC)
M68K_DEVICE ("5211",  mcf5211,  "5213",  "5208",  cfv2,     isa_aplus, FL_CF_HWDIV | FL_CF_MAC)
M68K_DEVICE ("5212",  mcf5212,  "5213",  "5208",  cfv2,     isa_aplus, FL_CF_HWDIV | FL_CF_MAC)
M68K_DEVICE ("5213",  mcf5213,  "5213",  "5208",  cfv2,     isa_aplus, FL_CF_HWDIV | FL_CF_MAC)
M68K_DEVICE ("5214",  mcf5214,  "5216",  "5208",  cfv2,     isa_aplus, FL_CF_HWDIV | FL_CF_EMAC)
M68K_DEVICE ("5216",  mcf5216,  "5216",  "5208",  cfv2,     isa_aplus, FL_CF_HWDIV | FL_CF_EMAC)
M68K_DEVICE ("5221x", mcf5221x, "5221x", "5208",  cfv2,     isa_aplus, FL_CF_HWDIV | FL_CF_MAC)
M68K_DEVICE ("52221", mcf52221, "52223", "5208",  cfv2,     isa_aplus, FL_CF_HWDIV | FL_CF_MAC)
M68K_DEVICE ("52223", mcf52223, "52223", "5208",  cfv2,     isa_aplus, FL_CF_HWDIV | FL_CF_MAC)
M68K_DEVICE ("52230", mcf52230, "52235", "5208",  cfv2,     isa_aplus, FL_CF_HWDIV | FL_CF_EMAC)
M68K_DEVICE ("52231", mcf52231, "52235", "5208",  cfv2,     isa_aplus, FL_CF_HWDIV | FL_CF_EMAC)
M68K_DEVICE ("52232", mcf52232, "52235", "5208",  cfv2,     isa_aplus, FL_CF_HWDIV | FL_CF_EMAC)
M68K_DEVICE ("52233", mcf52233, "52235", "5208",  cfv2,     isa_aplus, FL_CF_HWDIV | FL_CF_EMAC)
M68K_DEVICE ("52234", mcf52234, "52235", "5208",  cfv2,     isa_aplus, FL_CF_HWDIV | FL_CF_EMAC)
M68K_DEVICE ("52235", mcf52235, "52235", "5208",  cfv2,     isa_aplus, FL_CF_HWDIV | FL_CF_EMAC)
M68K_DEVICE ("5224",  mcf5224,  "5225",  "5208",  cfv2,     isa_aplus, FL_CF_HWDIV | FL_CF_MAC)
M68K_DEVICE ("5225",  mcf5225,  "5225",  "5208",  cfv2,     isa_aplus, FL_CF_HWDIV | FL_CF_MAC)
M68K_DEVICE ("52252", mcf52252, "52259", "5208",  cfv2,     isa_aplus, FL_CF_HWDIV | FL_CF_EMAC)
M68K_DEVICE ("52254", mcf52254, "52259", "5208",  cfv2,     isa_aplus, FL_CF_HWDIV | FL_CF_EMAC)
M68K_DEVICE ("52255", mcf52255, "52259", "5208",  cfv2,     isa_aplus, FL_CF_HWDIV | FL_CF_EMAC)
M68K_DEVICE ("52256", mcf52256, "52259", "5208",  cfv2,     isa_aplus, FL_CF_HWDIV | FL_CF_EMAC)
M68K_DEVICE ("52258", mcf52258, "52259", "5208",  cfv2,     isa_aplus, FL_CF_HWDIV | FL_CF_EMAC)
M68K_DEVICE ("52259", mcf52259, "52259", "5208",  cfv2,     isa_aplus, FL_CF_HWDIV | FL_CF_EMAC)
M68K_DEVICE ("52274", mcf52274, "52277", "5208",  cfv2,     isa_aplus, FL_CF_HWDIV | FL_CF_EMAC)
M68K_DEVICE ("52277", mcf52277, "52277", "5208",  cfv2,     isa_aplus, FL_CF_HWDIV | FL_CF_EMAC)
M68K_DEVICE ("5232",  mcf5232,  "5235",  "5208",  cfv2,     isa_aplus, FL_CF_HWDIV | FL_CF_EMAC)
M68K_DEVICE ("5233",  mcf5233,  "5235",  "5208",  cfv2,     isa_aplus, FL_CF_HWDIV | FL_CF_EMAC)
M68K_DEVICE ("5234",  mcf5234,  "5235",  "5208",  cfv2,     isa_aplus, FL_CF_HWDIV | FL_CF_EMAC)
M68K_DEVICE ("5235",  mcf5235,  "5235",  "5208",  cfv2,     isa_aplus, FL_CF_HWDIV | FL_CF_EMAC)
M68K_DEVICE ("523x",  mcf523x,  "5235",  "5208",  cfv2,     isa_aplus, FL_CF_HWDIV | FL_CF_EMAC)
M68K_DEVICE ("5249",  mcf5249,  "5249",  "5206e", cfv2,     isa_a,     FL_CF_HWDIV | FL_CF_EMAC)
M68K_DEVICE ("5250",  mcf5250,  "5250",  "5206e", cfv2,     isa_a,     FL_CF_HWDIV | FL_CF_EMAC)
M68K_DEVICE ("5253",  mcf5253,  "5253",  "5206e", cfv2,     isa_a,     FL_CF_HWDIV | FL_CF_EMAC)
M68K_DEVICE ("5270",  mcf5270,  "5271",  "5208",  cfv2,     isa_aplus, FL_CF_HWDIV | FL_CF_EMAC)
M68K_DEVICE ("5271",  mcf5271,  "5271",  "5208",  cfv2,     isa_aplus, FL_CF_HWDIV)
M68K_DEVICE ("5272",  mcf5272,  "5272",  "5206e", cfv2,     isa_a,     FL_CF_HWDIV | FL_CF_MAC)
M68K_DEVICE ("5274",  mcf5274,  "5275",  "5208",  cfv2,     isa_aplus, FL_CF_HWDIV | FL_CF_EMAC)
M68K_DEVICE ("5275",  mcf5275,  "5275",  "5208",  cfv2,     isa_aplus, FL_CF_HWDIV | FL_CF_EMAC)
M68K_DEVICE ("5280",  mcf5280,  "5282",  "5208",  cfv2,     isa_aplus, FL_CF_HWDIV | FL_CF_EMAC)
M68K_DEVICE ("5281",  mcf5281,  "5282",  "5208",  cfv2,     isa_aplus, FL_CF_HWDIV | FL_CF_EMAC)
M68K_DEVICE ("5282",  mcf5282,  "5282",  "5208",  cfv2,     isa_aplus, FL_CF_HWDIV | FL_CF_EMAC)
M68K_DEVICE ("528x",  mcf528x,  "5282",  "5208",  cfv2,     isa_aplus, FL_CF_HWDIV | FL_CF_EMAC)

/* CFV3 processors.  */
M68K_DEVICE ("53011", mcf53011, "53017", "5329",  cfv3,     isa_aplus, FL_CF_HWDIV | FL_CF_EMAC)
M68K_DEVICE ("53012", mcf53012, "53017", "5329",  cfv3,     isa_aplus, FL_CF_HWDIV | FL_CF_EMAC)
M68K_DEVICE ("53013", mcf53013, "53017", "5329",  cfv3,     isa_aplus, FL_CF_HWDIV | FL_CF_EMAC)
M68K_DEVICE ("53014", mcf53014, "53017", "5329",  cfv3,     isa_aplus, FL_CF_HWDIV | FL_CF_EMAC)
M68K_DEVICE ("53015", mcf53015, "53017", "5329",  cfv3,     isa_aplus, FL_CF_HWDIV | FL_CF_EMAC)
M68K_DEVICE ("53016", mcf53016, "53017", "5329",  cfv3,     isa_aplus, FL_CF_HWDIV | FL_CF_EMAC)
M68K_DEVICE ("53017", mcf53017, "53017", "5329",  cfv3,     isa_aplus, FL_CF_HWDIV | FL_CF_EMAC)
M68K_DEVICE ("5307",  mcf5307,  "5307",  "5307",  cfv3,     isa_a,     FL_CF_HWDIV | FL_CF_MAC)
M68K_DEVICE ("5327",  mcf5327,  "5329",  "5329",  cfv3,     isa_aplus, FL_CF_HWDIV | FL_CF_EMAC)
M68K_DEVICE ("5328",  mcf5328,  "5329",  "5329",  cfv3,     isa_aplus, FL_CF_HWDIV | FL_CF_EMAC)
M68K_DEVICE ("5329",  mcf5329,  "5329",  "5329",  cfv3,     isa_aplus, FL_CF_HWDIV | FL_CF_EMAC)
M68K_DEVICE ("532x",  mcf532x,  "5329",  "5329",  cfv3,     isa_aplus, FL_CF_HWDIV | FL_CF_EMAC)
M68K_DEVICE ("5372",  mcf5372,  "5373",  "5329",  cfv3,     isa_aplus, FL_CF_HWDIV | FL_CF_EMAC)
M68K_DEVICE ("5373",  mcf5373,  "5373",  "5329",  cfv3,     isa_aplus, FL_CF_HWDIV | FL_CF_EMAC)
M68K_DEVICE ("537x",  mcf537x,  "5373",  "5329",  cfv3,     isa_aplus, FL_CF_HWDIV | FL_CF_EMAC)

/* CFV4/CFV4e processors.  */
M68K_DEVICE ("5407",  mcf5407,  "5407",  "5407",  cfv4,     isa_b,     FL_CF_MAC)
M68K_DEVICE ("54410", mcf54410, "54418", "54455", cfv4,     isa_c,     FL_CF_HWDIV | FL_CF_USP | FL_CF_EMAC | FL_MMU | FL_UCLINUX)
M68K_DEVICE ("54415", mcf54415, "54418", "54455", cfv4,     isa_c,     FL_CF_HWDIV | FL_CF_USP | FL_CF_EMAC | FL_MMU | FL_UCLINUX)
M68K_DEVICE ("54416", mcf54416, "54418", "54455", cfv4,     isa_c,     FL_CF_HWDIV | FL_CF_USP | FL_CF_EMAC | FL_MMU | FL_UCLINUX)
M68K_DEVICE ("54417", mcf54417, "54418", "54455", cfv4,     isa_c,     FL_CF_HWDIV | FL_CF_USP | FL_CF_EMAC | FL_MMU | FL_UCLINUX)
M68K_DEVICE ("54418", mcf54418, "54418", "54455", cfv4,     isa_c,     FL_CF_HWDIV | FL_CF_USP | FL_CF_EMAC | FL_MMU | FL_UCLINUX)
M68K_DEVICE ("54450", mcf54450, "54455", "54455", cfv4,     isa_c,     FL_CF_HWDIV | FL_CF_USP | FL_CF_EMAC | FL_MMU | FL_UCLINUX)
M68K_DEVICE ("54451", mcf54451, "54455", "54455", cfv4,     isa_c,     FL_CF_HWDIV | FL_CF_USP | FL_CF_EMAC | FL_MMU | FL_UCLINUX)
M68K_DEVICE ("54452", mcf54452, "54455", "54455", cfv4,     isa_c,     FL_CF_HWDIV | FL_CF_USP | FL_CF_EMAC | FL_MMU | FL_UCLINUX)
M68K_DEVICE ("54453", mcf54453, "54455", "54455", cfv4,     isa_c,     FL_CF_HWDIV | FL_CF_USP | FL_CF_EMAC | FL_MMU | FL_UCLINUX)
M68K_DEVICE ("54454", mcf54454, "54455", "54455", cfv4,     isa_c,     FL_CF_HWDIV | FL_CF_USP | FL_CF_EMAC | FL_MMU | FL_UCLINUX)
M68K_DEVICE ("54455", mcf54455, "54455", "54455", cfv4,     isa_c,     FL_CF_HWDIV | FL_CF_USP | FL_CF_EMAC | FL_MMU | FL_UCLINUX)
M68K_DEVICE ("5470",  mcf5470,  "5475",  "5475",  cfv4e,    isa_b,     FL_CF_USP | FL_CF_EMAC | FL_CF_FPU | FL_MMU)
M68K_DEVICE ("5471",  mcf5471,  "5475",  "5475",  cfv4e,    isa_b,     FL_CF_USP | FL_CF_EMAC | FL_CF_FPU | FL_MMU)
M68K_DEVICE ("5472",  mcf5472,  "5475",  "5475",  cfv4e,    isa_b,     FL_CF_USP | FL_CF_EMAC | FL_CF_FPU | FL_MMU)
M68K_DEVICE ("5473",  mcf5473,  "5475",  "5475",  cfv4e,    isa_b,     FL_CF_USP | FL_CF_EMAC | FL_CF_FPU | FL_MMU)
M68K_DEVICE ("5474",  mcf5474,  "5475",  "5475",  cfv4e,    isa_b,     FL_CF_USP | FL_CF_EMAC | FL_CF_FPU | FL_MMU)
M68K_DEVICE ("5475",  mcf5475,  "5475",  "5475",  cfv4e,    isa_b,     FL_CF_USP | FL_CF_EMAC | FL_CF_FPU | FL_MMU)
M68K_DEVICE ("547x",  mcf547x,  "5475",  "5475",  cfv4e,    isa_b,     FL_CF_USP | FL_CF_EMAC | FL_CF_FPU | FL_MMU)
M68K_DEVICE ("5480",  mcf5480,  "5485",  "5475",  cfv4e,    isa_b,     FL_CF_USP | FL_CF_EMAC | FL_CF_FPU | FL_MMU)
M68K_DEVICE ("5481",  mcf5481,  "5485",  "5475",  cfv4e,    isa_b,     FL_CF_USP | FL_CF_EMAC | FL_CF_FPU | FL_MMU)
M68K_DEVICE ("5482",  mcf5482,  "5485",  "5475",  cfv4e,    isa_b,     FL_CF_USP | FL_CF_EMAC | FL_CF_FPU | FL_MMU)
M68K_DEVICE ("5483",  mcf5483,  "5485",  "5475",  cfv4e,    isa_b,     FL_CF_USP | FL_CF_EMAC | FL_CF_FPU | FL_MMU)
M68K_DEVICE ("5484",  mcf5484,  "5485",  "5475",  cfv4e,    isa_b,     FL_CF_USP | FL_CF_EMAC | FL_CF_FPU | FL_MMU)
M68K_DEVICE ("5485",  mcf5485,  "5485",  "5475",  cfv4e,    isa_b,     FL_CF_USP | FL_CF_EMAC | FL_CF_FPU | FL_MMU)
M68K_DEVICE ("548x",  mcf548x,  "5485",  "5475",  cfv4e,    isa_b,     FL_CF_USP | FL_CF_EMAC | FL_CF_FPU | FL_MMU)

/* Fido processor.  */
M68K_DEVICE ("fidoa", fidoa,    "cpu32", "fidoa", cpu32,    isa_cpu32, FL_FIDOA | FL_MMU)
</pre></body></html>